{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["乐器及教室设备清单","音乐厅交响厅设备清单"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"乐器及教室设备清单","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"merged":[[0,0,0,5],[2,1,13,1]],"flags":["formulas_cached_only"]}
["  "]
["编号","项目     分类","项目明细","数量","日期（2015年）","备注"]
[1,"演出教学乐器及舞台设备","爵士鼓",2,"10月12-16日","收藏家Collector22、18、16、14、12、10配套支架及REMO鼓皮（美产）枫木10层套鼓；配件及鼓皮需全美产；pdp小尺寸枫木爵士专业用鼓"]
[2,null,"镲片",1,"10月12-16日","镲片：K dark;KC dark;A series；sabianAAX"]
[3,null,"爵士吉他音箱",1,"10月12-16日","爵士吉他音箱：晶体管吉他音箱输出功率60－120W"]
[4,null,"爵士吉他音箱",2,"10月12-16日","爵士吉他音箱：电子管前级及后级；吉他箱体：jensen喇叭；输出功率120W"]
[5,null,"分体吉他音箱",2,"10月12-16日","分体吉他音箱：全管分体吉他音箱；412；150W；需直角开关型"]
[6,null,"主键盘",1,"10月12-16日","主键盘88键"]
[7,null,"副主键盘",1,"10月12-16日","主键盘88键"]
[8,null,"教学用爵士鼓",1,"10月12-16日","教学用鼓22141210配有22寸Delite及S Classix混装套鼓桦木 德产"]
[9,null,"贝斯分体音箱",1,"10月12-16日","贝斯音箱：前级电子管后级晶体管低音音箱"]
[10,null,"贝斯分体演唱会音箱",1,"10月12-16日","贝斯音箱：数字放大前级低音音箱（倍数倍率）"]
[11,null,"教室扩声系统",3,"10月12-16日","3只为ABC三点式开角55度；MS制式立体声；需搭配CAF215分频低音（附phonic分频器）"]
[12,null,"数控模拟调音台",2,"10月12-16日","1644Ai：16话放8线放数控模拟调音台；可存储及编程"]

{"sheet":"音乐厅交响厅设备清单","index":1,"n_rows":28,"n_cols":6,"rows_kept":28,"merged":[[0,0,0,5],[2,1,24,1],[25,1,27,1]],"flags":["formulas_cached_only"]}
["  "]
["编号","项目     分类","项目明细","数量","日期（2015年）","备注及需求"]
[1,"音频类设备","PZM180度开角底鼓话筒",1,"10月12-16日","PZM制式180度开角可悬挂电容传声器"]
[2,null,"动圈底鼓话筒",1,"10月12-16日","大振膜动圈低鼓传声器（dr：117dB）"]
[3,null,"动圈军鼓35度开角话筒",1,"10月12-16日","35度开角传声器"]
[4,null,"动圈爵士专用Tom鼓话筒",4,"10月12-16日","爵士专用中低频传声器"]
[5,null,"大振膜电容OH话筒或打击乐",4,"10月12-16日","大振膜电容话筒需德产原装"]
[6,null,"钢琴贴片履带式电容话筒",2,"10月12-16日","钢琴贴片履带式浮共振板电容传声器"]
[7,null,"小振膜锐心型话筒",1,"10月12-16日","小振膜锐心型高阻抗传声器"]
[8,null,"动圈乐器拾音话筒",3,"10月12-16日","动圈乐器传声器"]
[9,null,"无线人声系统及无线监听",8,"10月12-16日","无线人声系统及IEM"]
[10,null,"人声手持动圈话筒",4,"10月12-16日","人声手持动圈话筒"]
[11,null,"四通道数模转换器",2,"10月12-16日","欧姆阻抗转换盒（带输入牛输出牛放大）均携带150－600欧姆的主动式转换"]
[12,null,"信号缆车",1,"10月12-16日","平衡信号 32进8出 lappkable(德国)"]
[13,null,"耳机分配器",1,"10月12-16日","无线IEM耳机监听接收器及信号增强器"]
[14,null,"线材","N","10月12-16日","caname及monster（neutrik接头）"]
[15,null,"麦架",30,"10月12-16日","长短折"]
[16,null,"主扩系统",1,"10月12-16日","RCF线阵列16中程3＊218低音（法国）；双八寸单元开角120度单列8只聚焦17米；218呈ABC制式（需搭配独立分频处理器）规格：二分频全频音箱，频响：80Hz-20kHz（±3dB），号角辐射角度：120°Hor.×7°Vert.，单元：2X8寸(200mm)低频单元，1X1.4\"(34mm)高频单元；额定功率：中低音：300W，高音：100W；最大功率(PEAK):中低音：1200W，高音：400W；额定阻抗：高音：8欧姆，中低音：16欧姆；灵敏度：中低音：98dB，高音：108dB；最大长期声压级：中低音：126dB，高音：131dB；尺寸：高252mm×宽680mm×深460mm；重量：26kg；规格：远程超低音箱；频响：40Hz～300Hz(±3dB)，单元：2X18\"(460mm)低频单元；额定功率：1600W，；最大功率(PEAK)：6400W；额定阻抗：4 ohm；灵敏度：105dB；最大长期声压级：138dB；尺寸：高530mm×宽1078mm×深695mm；重量：95kg"]
[17,null,"监听系统",8,"10月12-16日","单12、15返听系统450w（Proel及KH）可做多开角调整"]
[18,null,"Truss架搭建",204,"10月12-16日","全舞台Truss架搭建用于灯光及声学L17;W12;H9"]
[19,null,"数字调音台",1,"10月12-16日","32路16编组＋S16＊2；搭配网络数字盒的40输入16输出需佩带WAVES APA32扩展处理器"]
[20,null,"ledpar灯",16,"10月12-16日","led灯 PAR-64 GENERAL LIGHT 220V(1000W)"]
[null,null,"追光灯",2,"10月12-16日","追光（含人工）"]
[21,null,"电脑光束灯Beam",24,"10月12-16日","编程光束灯含面光 EAGLE-1200 MOVE LIGHT(1200W)"]
[22,null,"灯控台",1,"10月12-16日","Pearl 2000控台"]
[23,"人工","调音师",2,"10月12-16日","专业音乐学院录音艺术专业本科文凭"]
[24,null,"灯光师",2,"10月12-16日"]
[25,null,"音响工程人员",15,"10月12-16日"]